START server

While True:

LISTEN for incoming connections

If there is incoming connection from user or admin:

ACCEPT connection

CREATE client thread

While True:

RECEIVE incoming data from client

READ data and call the corresponding function

If incoming data is a call to exit thread:

Break

END thread